FRAME HEADER FRAMEPAYLOADAREA

DATAGRAM HEADER DATAGRAMPAYLOADAREA

UDP HEADER UDP PAYLOAD

Figure 10.6 Two levels of encapsulation used when a UDP message travels in an IP datagram, which travels in a network frame.