(application closes connection) Send FINseq=x

Receive FINsegment Send ACKx+1 (inform application) Receive ACKsegment

(application closes connection) Send FINseq=y, ACKx+1

Receive FIN+ ACKsegment Send ACKy+1

Receive ACKsegment

Events At Site 1 Network Messages Events At Site 2

Figure 11.15 The three-way handshake used to close a connection with an extra ACK sent immediately upon receipt of a FIN.