Destination Distance Route Net1 Net2 Net4 Net17 Net24 Net30 Net42

0 0 8 5 6 2 2 direct direct Router L Router M Router J Router Q Router J

Destination Distance Net1 Net4 Net17 Net21 Net24 Net30 Net42

2 3 6 4 5 10 3 (a) (b)

Figure 12.5 (a) An existing FIB in router K, and (b) an incoming routing update message from router J that will cause changes.