0 7 15

Address Family Family Extension Addr. Length Next Hop Address (variable)

. . .

Num. of SNPAs, N Length of SNPA1 SNPA 1 (variable)

. . .

Length of SNPA2 SNPA 2 (variable)

. . . . . Length of SNPA N SNPAN(variable)

. . .

Network Layer Reachability Information (variable)

. . .

Figure 13.14 The format of a BGP Multiprotocol Reachable NLRI attribute used for IPv6 and other non-IPv4 destination addresses.