0 8 31

LEN IPv4 Address Prefix (1-4octets)

Figure 13.7 The compressed format BGP uses to store an IPv4 destination address and the associated address mask.