0 1 2 3 4 5 6 7 8 15

Flag Bits Type Code (a) Flag Bits Description 0 1 2 3 5-7

0 for required attribute, 1 if optional 1 for transitive, 0 for nontransitive 0 for complete, 1 for partial 0 if length field is one octet, 1 if two unused (must be zero) (b)

Figure 13.8 (a) The two-octet type field that appears before each BGP attribute path item, and (b) the meaning of each flag bit.