0 8 16 24 31

OSPF HEADERWITHTYPE=1

NETWORKMASK HELLOINTERVAL OPTIONS GWAYPRIO ROUTERDEADINTERVAL DESIGNATEDROUTER BACKUPDESIGNATEDROUTER NEIGHBOR_1 IP ADDRESS NEIGHBOR_2 IP ADDRESS . . .

NEIGHBOR_n IP ADDRESS

Figure 14.10 The OSPFv2 hello message format. A pair of neighbor routers exchanges hello messages periodically to test reachability.