0 16 31

OSPF HEADERWITHTYPE=3

LS TYPE LINKID ADVERTISINGROUTER . . .

Figure 14.12 OSPFv2 link-status request message format. A router sends the message to a neighbor to request current information about a specific set of links.