0 16 31

OSPF HEADERWITHTYPE=4

NUMBEROF LINKSTATUSADVERTISEMENTS

LINKSTATUSADVERTISEMENT_1

. . .

LINKSTATUSADVERTISEMENT_n

Figure 14.13 OSPFv2 link-status update message format. A router sends such a message to broadcast information about its directly connected links to all other routers.