0 8 16 24 31

OSPFv3 HEADERWITHTYPE=1

INTERFACEID ROUTERPRIO OPTIONS HELLOINTERVAL ROUTERDEADINTERVAL DESIGNATEDROUTERID BACKUPDESIGNATEDROUTERID NEIGHBOR_1 ID NEIGHBOR_2 ID . . .

NEIGHBOR_n ID

Figure 14.16 The OSPFv3 hello message format. All IPv4 addresses have been replaced by 32-bit identifiers.