R_2

R_1

R_4

R_3

R_5

Net 2

Net 3

Net 1

Net 4 Net 5

Figure 14.2 The addition of router R_5 introduces an alternate path between networks 2 and 3. Routing software can quickly adapt to a failure and automatically switch routes to the alternate path.