BGP used

R_1 R_2

Autonomous System 1

Autonomous System 2

IGP_1 used

IGP_2 used

Figure 14.3 Conceptual view of two autonomous systems, each using its own IGP internally, and then using BGP to communicate routes to another system.