0 8 16 24 31

COMMAND(1–5) VERSION(2) MUSTBE ZERO FAMILYOF NET1 ROUTETAGFOR NET1 IP ADDRESSOF NET1 SUBNETMASKFORNET1 NEXTHOP FORNET1 DISTANCETONET1 FAMILYOF NET2 ROUTETAGFOR NET2 IP ADDRESSOF NET2 SUBNETMASKFORNET2 NEXTHOP FORNET2 DISTANCETONET2 . . .

Figure 14.5 The format of an IPv4 version 2 RIP message. After the 32-bit header, the message contains a sequence of pairs, where each pair specifies an IPv4 prefix, next hop, and distance to the destination.