0 8 16 31

COMMAND(1-2) VERSION(1) MUSTBE ZERO

ROUTETABLEENTRY1 (20 OCTETS)

ROUTETABLEENTRY N (20 OCTETS) . . . .

Figure 14.7 The overall format of a RIPng message used to carry IPv6 routing information.