0 8 16 24 31

VERSION(2) TYPE MESSAGELENGTH SOURCEROUTERIP ADDRESS AREAID CHECKSUM AUTHENTICATIONTYPE AUTHENTICATION(octets 0–3) AUTHENTICATION(octets 4–7)

Figure 14.9 The fixed 24-octet OSPFv2 header that appears in each message.