0 8 16 31

TYPE(130) CODE(0) CHECKSUM

MAXIMUMRESPONSE CODE RESERVED

SPECIFICMULTICASTADDRESS OR ZEROFOR AGENERALQUERY

RESV S QRV QQIC NUMBEROFSOURCES (N)

SOURCE 1 ADDRESS

. .

SOURCE N ADDRESS

Figure 15.12 The format of an MLDv2 query message. A multicast router sends such messages to determine whether hosts on a network are participating in multicast.