FRAME HEADER

FRAMEPAYLOAD

MPLS HDR MPLSPAYLOAD

DATAGRAM HEADER

DATAGRAMPAYLOAD

Figure 16.3 The encapsulation used with MPLS to send an IPv4 datagram over a conventional network, such as an Ethernet. An MPLS header is variable size, and depends on the number of entries in the label stack.