. . .

Traditional Stack

Label Switching Code

Apps (Layer 5)

TCP(Layer 4)

IP (Layer 3)

Classifier

MPLSModule

interface 1 interface 2 interface N

net 1 net 2 net N ...

Figure 17.3 Layering when a router uses classification to select MPLS paths.