... 6 octets 6 octets 4 octets 2 octets 46–1500 octets

Destination Address

Source Address

VLAN Tag Frame Type Frame Payload (Data)

Figure 17.4 Illustration of an IEEE 802.1Q VLAN tag field inserted in an Ethernet frame after the frame arrives at a VLAN switch.