* * * * * * * * * * * *^{08 00} * * * * ...

00 24 e8 3a b1 f1 00 24 e8 3a b2 6a 08 06 00 01 08 00 ...

00 24 e8 3a b2 6a 00 24 e8 3a b1 f1 08 00 45 00 00 28 ...

(a) Apattern shown in hexadecimal

(b) Aframe carrying an ARPreply

(c) Aframe carrying an IP datagram

Figure 17.7 (a) A pattern in a TCAM with asterisks indicating “don’t care”, (b) an ARP packet that does not match the pattern, and (c) an IP datagram that matches the pattern.