INTERNET

R_1

R_2

R_3

R_4

128.10.1.0/24

128.10.2.0/24

192.5.48.0/24

128.210.0.0/16

Site 1 Site 2

Forwarding table in router R_1 destination next hop 128.10.1.0/24 direct 128.10.2.0/24 R_2 192.5.48.0/24 tunnel to R_3 128.210.0.0/16 tunnel to R_3 default ISP’s router

Figure 19.3 A VPN that spans two sites and R_1’s forwarding table with a VPN tunnel from R_1 to R_3 configured like a point-to-point circuit.