. . . 6 octets 6 octets 2 octets 46–1500 octets

Destination Address

Source Address

Frame Type Frame Payload (Data)

Figure 2.2 Ethernet frame format. Fields are not drawn to scale.