MUSTBE ZERO B

0 15

Figure 22.2 The format of the 16-bit FLAGS field in a DHCP message. The leftmost bit is interpreted as a broadcast request; all others bits must be set to zero.