IP HEADER TCP HEADER TCP DATA

IP HEADER ESP HEADER TCP HEADER TCP DATA ESP TRAILER ESP AUTH

(a)

(b) encrypted authenticated

Figure 29.3 (a) A datagram, and (b) the same datagram using IPsec Encapsulating Security Payload. Intermediate routers can only interpret unencrypted fields.