Demultiplexing Based On Frame Type

ARP Module

IP Module RARPModule

Frame Arrives

Figure 4.10 Illustration of frame demultiplexing that uses a type field in the frame header. Demultiplexing is used with most networks, including Ethernet and Wi-Fi.