64 zero bits 16 bits 16 bits 32 bits 0000 . . . . . . . . . . . . . 0000 0000 FFFF IPv4 Address 0000 . . . . . . . . . . . . . 0000 FFFF 0000 IPv4 Address

Figure 5.12 Two ways to embed an IPv4 address in an IPv6 address. The second form is used for Stateless IP/ICMP Translation.