GLOBALROUTINGPREFIX SUBNETID INTERFACEID

N bits 64–Nbits 64 bits

Figure 5.13 The division of an IPv6 unicast address into three conceptual parts. The interface ID always occupies 64 bits.