        0 47

               8 24

0 63

       8 24 40

c cc c cc 0gc cc cc c cc cc c cc cc c

c cc c cc 1gc cc cc c cc cc c cc cc c 1111111111111110

extension

extension

(a)

(b)

Figure 5.14 (a) The format of a 48-bit Ethernet address, with bits that identify a manufacturer and extension, and (b) the address when placed in the low-order 64 bits of an IPv6 unicast address.