all 0s all 1s net all 1s net all 0s net subnet all 1s 127 anything (often 1) 14 multicast group ID

Startup source address Limited broadcast (local net) Directed broadcast for net Network address Nonstandard directed broadcast Subnet broadcast Loopback Multicast address

Figure 5.15 Summary of IPv4 special addresses.