R_1 R_2

ETHERNET 128.10.0.0/16

WI-FI NETWORK 128.210.0.0/16 ISP 9.0.0.0/8

routers

Figure 5.17 Example architecture of a site with IPv4 address prefixes assigned to two networks.