Internet portion physical network host

16 bits 10 bits 6 bits

Figure 5.5 A division of a 16-bit local portion that accommodates 400 networks.