0 8 16 24 31

HARDWARETYPE PROTOCOLTYPE HLEN PLEN OPERATION SENDERHARD(octets 0-3) SENDERHARD(octets 4-5) SENDERIPv4 (octets 0-1) SENDERIPv4 (octets 2-3) TARGETHARD(octets 0-1) TARGETHARD(octets 2-5) TARGETIPv4 (octets 0-3)

Figure 6.4 The ARP message format when used to map an IPv4 address to an Ethernet address.