0 4 8 16 19 24 31

VERS HLEN SERVICETYPE TOTALLENGTH IDENTIFICATION FLAGS FRAGMENTOFFSET TIMETOLIVE PROTOCOL HEADERCHECKSUM SOURCEIP ADDRESS DESTINATIONIP ADDRESS IP OPTIONS(IFANY) PADDING PAYLOAD . . .

Figure 7.3 Format of an IPv4 datagram, the basic unit of transfer in a TCP/IP internet.