0 4 12 16 24 31

VERS TRAFFICCLASS FLOWLABEL PAYLOADLENGTH NEXTHEADER HOP LIMIT

SOURCEADDRESS

DESTINATIONADDRESS

Figure 7.6 The IPv6 base header format; the size is fixed at 40 octets.