Host

R_1 R_2 path to some destinations path to other destinations

Figure 8.1 An example of a singly-homed host that must make a choice between router R_1 and router R_2 when sending a datagram.