Datagrams with Dst=200

Datagrams with Dst=210

UDP input appl. 1 appl. 2

Dst=200 Src=397; 192.5.48.3

Dst=200 Src=40;

128.10.2.26

Dst=210 Src=502; 128.10.3.30

Dst=200 Src=ANY appl. 1 appl. 2 appl. 3 appl. 4

UDP input

(a) operating system

(b)

Figure 10.2 The two styles of UDP demultiplexing: (a) using only destination port, and (b) using (source, destination) port pairs. In style (a), an application receives all datagrams to a given destination port. In style (b) it only receives datagrams from the specified source.