IP Process

TCPInput Process

port for segments sent to TCP bufferscontrolled bysemaphores ports for UDP datagrams

Figure 2.3 The flow of datagrams through higher layers of software. The IP process sends incoming segments to the TCP process, but places incoming UDP datagrams directly in separate ports where they can be accessed by application programs.