R_1

INTERNET R_2 R_3 M D Home Site Foreign Site

mobile host destination

mobile’s original home home agent

Figure 18.5 A topology in which mobile IPv4 routing is incredibly inefficient. When a mobile host, M, communicates with a local destination, D, replies from D travel across the Internet to the mobile’s home agent, R_1, and then back to the mobile host.