REBIND

INITIALIZE

BOUND

RENEW

SELECT

REQUEST

/DHCPDISCOVER

Select Offer/ DHCPREQUEST

DHCPOFFER

DHCPACK

DHCPACK

DHCPACK

DHCPNACK

DHCPNACK or Lease Expires

Lease Reaches 50% Expiration / DHCPREQUEST

Lease Reaches 87.5% Expiration / DHCPREQUEST

Host Boots

Cancel Lease /DHCPRELEASE

Figure 22.3 The six main states of a DHCP client and transitions among them. Each label on a transition lists the incoming message or event that causes the transmission, followed by a slash and the message the client sends.