PDU::= CHOICE{ get-request

GetRequest-PDU, get-next-request GetNextRequest-PDU, get-bulk-request GetBulkRequest-PDU, response

Response-PDU, set-request

SetRequest-PDU, inform-request InformRequest-PDU, snmpV2-trap SNMPv2-Trap-PDU, report

Report-PDU, }

Figure 27.10 The ASN.1 definitions of an SNMP PDU. The syntax for each request type must be specified further.