not yet sent (part 2) sent but not acknowledged not yet sent (part 1) unused buffer space

. . . . . . .

sbcount bytes

sbstart sbsize end

Figure 13.4 Available data wrapped around a circular TCP output buffer. Variable sbcount tells the number of available bytes and end gives the location of the last byte of data. End can be computed as (sbstart+sbcount) mod sbsize.